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Datasets description
This data set is aimed at the qiaogori peak area, including the glacier and surrounding areas in the chogori peak area, and the digital elevation model of the area in 2013 obtained by using remote sensing images. The data set contains one band, and the complex data of the same ground object can be obtained by using the platform equipped with synthetic aperture radar sensor at the same time or two parallel observations. After accurate registration, complex interferograms can be obtained by conjugate multiplication of complex images. Based on the geometric relationship among flight platform, beam view and baseline, the digital elevation model of glacier area is obtained by unwrapping the phase information of complex interferogram. Only for the glacier surface elevation in 2013, so it will not be supplemented and improved, and fully open sharing is adopted. The data set contains dem2013, a total of 1 band. Data set file name and band name are as follows: data set file name: 2013 qiaogori peak area digital elevation model data set, dem2013-2013 digital elevation model of this area, unit: meter (m). 
Data source description
This data set is mainly interpreted data, and the main data source is TerraSAR-X / TanDEM-X microwave remote sensing data.
Data processing method
The complex data of the same object on the ground can be obtained by using the platform equipped with synthetic aperture radar (SAR) sensor and observing at the same time or twice in parallel. After accurate registration, complex interferograms can be obtained by conjugate multiplication of complex images. Based on the geometric relationship among flight platform, beam view and baseline, the digital elevation model of glacier area is obtained by unwrapping the phase information of complex interferogram.
Data quality description
By using the platform equipped with TerraSAR-X and TanDEM-X sensors, the complex data (including amplitude and phase information) of the same ground object are obtained at the same time to form an interference pair. After accurate registration, complex interferograms can be obtained by conjugate multiplication of complex images. Based on the geometric relationship among flight platform, beam view and baseline, the phase information in complex interferogram is unwrapped to obtain the ground elevation information. The absolute accuracy in the vertical direction is better than 10 m, and the relative accuracy is 4 m at & gt; 20% and 2 m at & lt; 20%. 
Base information
collect time:2013/02/01-2013/02/28
collect place:chogori peak 
data size:567.9 KiB
data format:
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Citations and annotations
In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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