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Datasets description
 
Data source description
Continuous observation by instrument and regular observation manually
Data processing method
<p>There are SM1 rain gauge with diameter of 20cm and dsj2 siphon self recording rain gauge. SM1 adopts 8:00 and 20:00 two-stage system for annual observation, mainly observing the beginning and ending time of precipitation, and counting the precipitation. When the intermittent time of precipitation is more than 15 min, it is observed as two precipitation before and after the interval. When the intermittent time is less than 15 min, it is regarded as a precipitation observation record. If a precipitation crosses 8:00 and 20:00, it should be measured at 8:00 and 20:00. Dsj2 adopts 24 segment system for flood season observation. In case of failure of self recording rain gauge, the observation data of ordinary rain gauge are supplemented. </p>
Data quality description
The recording rain gauge shall be calibrated before the start of observation every year. In the process of data entry, there are four levels of manual verification: tabulation, initial verification, re verification, and audit to ensure data quality 
Base information
collect time:2024/01/01-2024/12/31
collect place:Jiuyuangou Valley, Jiuyuangou Township, Suide County, Yulin City, Shaanxi Province 
data size:315.5 KiB
data format:excel,word,pdf
Coordinate system: WGS84 
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contacts:Min Yu Fang 
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Contact information
contributors:Suide administration and Supervision Bureau of water and soil conservation of the Yellow River (Suide scientific experimental station of water and soil conservation) 
author:Suide administration and Supervision Bureau of water and soil conservation of the Yellow River (Suide scientific experimental station of water and soil conservation)  
manager:Suide administration and Supervision Bureau of water and soil conservation of the Yellow River (Suide scientific experimental station of water and soil conservation) 
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Citations and annotations
In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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