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Datasets description
<p>This data set is the precipitation observation data from four rainfall stations (yingfangliang, experimental field, qiaozigou mouth, Malan) in the third sub region of Loess Hilly and gully region from 1991 to 2000. SM1 ordinary rain gauge and SL-1 self recording rain gauge are used for observation. This data set includes daily precipitation scale, precipitation extract table, maximum precipitation scale (1) and precipitation observation results of successive floods. </p> 
Data source description
<p>Instrument continuous observation; manual timing observation; manual data extraction and compilation</p>
Data processing method
<p>SM1 ordinary rain gauge is used for annual observation, which is extracted in flood season (from May to October) in 4-stage system and 2-stage system in non flood season; SL-1 self recording rain gauge is used for flood season observation with 24 segment system. The self recording rain gauge is calibrated before the flood season, and the abnormal value in the observation process is interpolated with the observation value of ordinary rain gauge. </p>
Data quality description
<p>The precipitation observation data shall be observed, sorted and compiled in strict accordance with the provisions of "precipitation observation specification" (SL21). Observation data shall be measured, calculated, sorted and analyzed in accordance with the requirements of "four follow-up". Errors and unreasonable records of observation shall be handled and corrected in time, and remarks shall be made. During the compilation and input of observation data, four levels of manual verification (tabulation, primary calibration, re calibration and audit) are carried out to ensure the data quality. </p> 
Base information
collect time:1991/01/01-2000/12/31
collect place:Qiaozigou watershed, Qinzhou District, Tianshui City, Gansu Province 
altitude:1666.5m- 1235.0m
data size:526.8 KiB
data format:
Coordinate system: 无 
Keywords
Theme:Annual rainfall, daily rainfall, interval rainfall, maximum rainfall, rainfall extract, qiaozigou basin
	Subject:
	Time:1990 1991 1992 1993 1994 1995 1996 1997 1998 1999
	Place:Tianshui,  qiaozigou,  Gansu Province 
Space scope
	
	north： 34.66
	

	west：105.51
	
	east：105.74

	
	south： 34.59
	


Service information
contacts:Min Yufang 
phone:0931-4967596
mailbox:ncdc@lzb.ac.cn
Contact information
contributors: 
author:Liu Xiao  
manager: 
Project information

Citations and annotations
In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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