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Datasets description
This data set includes 5.5km of Yingke / Daman irrigation area in the middle reaches of Heihe River × Continuous observation data set of 75 bnunet nodes in the 5.5km observation matrix from May to September 2012. The configuration of 75 nodes is the same, including 3-layer soil temperature probes at the depth of 4cm, 10cm and 20cm and 1-layer soil moisture probe at the depth of 4cm. The observation frequency is 10 minutes. This data set can provide a spatio-temporal continuous observation data set for remote sensing estimation and remote sensing authenticity test of key hydrothermal variables on heterogeneous surface, eco hydrological research, irrigation optimization management and so on. The time is UTC + 8. For details, see "bnunet data document. Docx". 
Data source description
   This data set can provide a spatio-temporal continuous observation data set for remote sensing estimation and remote sensing authenticity test of key hydrothermal variables on heterogeneous surface, eco hydrological research, irrigation optimization management and so on. The time is UTC + 8.
Data processing method
   The configuration of 75 nodes is the same, including 3-layer soil temperature probes at the depth of 4cm, 10cm and 20cm and 1-layer soil moisture probe at the depth of 4cm. The observation frequency is 10 minutes.
Data quality description
   Good data quality 
Base information
collect time:2012/05/12-2012/09/16
collect place:Heihe River Basin, middle reaches, artificial oasis, experimental area 
data size:49.8 MiB
data format:
Coordinate system: WGS84 
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