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Datasets description
& emsp; This dataset consists of 25 runoff fields in the Nanxiaohegou watershed in 2023, including 14 bare land slope zones with 7 measurement points, 6 forest land with 4 measurement points, 5 natural barren slope zones with 5 measurement points, and 35 runoff fields in 2020 with 14 bare land slope zones with 7 measurement points, 6 forest land with 4 measurement points, 6 natural barren slope zones with 6 measurement points, and 10 artificial grassland with 10 measurement points for soil moisture content observation. Between April and October, soil drills are used to collect samples in layers within the community protection zone on the 1st, 11th, and 21st of each month. Samples are taken from each layer at depths of 0-10cm, 10-20cm, 20-40cm, 40-60cm, 60-80cm, and 80-100cm. The soil moisture content is measured using the TDR method, which represents the soil moisture content of the soil layer. After rainfall and runoff, soil moisture is also measured after rainfall 
Data source description
 TDR instrument observation
Data processing method
 Instrument directly reads data
Data quality description
 Observations are compiled and entered through four levels of manual checking, namely, tabulation, initial checking, rechecking, and auditing, to ensure the quality of the data. 
Base information
collect time:2024/01/01-2024/12/31
collect place:South Xiaohegou Basin, Houguanzhai Township, Xifeng District, Qingyang City, Gansu Province 
altitude:1050.0m- 1423.0m
data size:108.5 KiB
data format:
Coordinate system: WGS84 
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Theme:Soil moisture content of each sampling depth
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For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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