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Datasets description
 
Data source description
Instrument continuous observation and manual timing observation
Data processing method
Precipitation observation instruments include dsj2 siphon rain gauge and SM1 ordinary rain gauge with diameter of 20cm. Dsj2 self recording rain gauge adopts 24 segment system for flood season observation, SM1 ordinary rain gauge adopts 8:00 and 20:00 two-stage system for annual observation. In case of failure of self recording rain gauge, observation data of ordinary rain gauge are used for supplement. It mainly observes the beginning and ending time of precipitation and statistics of precipitation. When the intermittent time of precipitation is more than 15min, it is observed as two precipitation before and after the interval. When the intermittent time is less than 15min, it is recorded as a precipitation observation. If a precipitation crosses 8:00 and 20:00, it should be measured at 8:00 and 20:00.
Data quality description
The instrument calibration shall be carried out before the start of annual observation of rain gauge. In the process of data entry, there are four levels of manual verification, including tabulation, primary proofreading, rechecking and auditing, so as to ensure the data quality. 
Base information
collect time:1986/01/01-1990/12/31
collect place:Qiaogou watershed, Suide County, Yulin City, Shanxi Province 
data size:496.7 KiB
data format:xls，doc，pdf
Coordinate system: WGS84 
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The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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