Basic situation of farmland runoff field in liangjiaping, daliushugou, the third sub region of Loess Hilly and gully region, 1945-1957
DOI：10.12072/ncdc.HWTSZhan.db0014.2020
CSTR：11738.11.ncdc.HWTSZhan.2020.42
Share type:Apply to Access
Category:Soil and Water Conservation
Datasets description
 
Data source description

Data processing method

Data quality description
 
Base information
collect time:1945/01/01-1957/01/01
collect place:
altitude:2.0m- Nonem
data size:975.0 KiB
data format:
Coordinate system: WGS84 
Projection  
Keywords
Theme:Runoff coefficient, runoff depth, erosion modulus, sediment content, runoff modulus, soil loss, runoff, flow, water level, sediment transport rate
	Subject:
	Time:1945 1946 1947 1948 1949 1950 1951 1952 1953 1954 1955 1956 1957
	Place:Gansu 
Space scope
	
	north： 35.00
	

	west：105.90
	
	east：105.92

	
	south： 34.96
	


Service information
contacts: 
phone:0931-4967596
mailbox:ncdc@lzb.ac.cn
Contact information
contributors: 
author:Liu Xiao  
manager: 
Project information

Citations and annotations
In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
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The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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