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Datasets description
 
Data source description
Instrument continuous observation, artificial timing observation
Data processing method
There are SM1 rain gauge with diameter of 20cm and dsj2 siphon self recording rain gauge. SM1 adopts 8:00 and 20:00 two-stage system for annual observation, mainly observing the beginning and ending time of precipitation, and counting the precipitation. When the intermittent time of precipitation is more than 15 min, it is observed as two precipitation before and after the interval. When the intermittent time is less than 15 min, it is regarded as a precipitation observation record. If a precipitation crosses 8:00 and 20:00, it should be measured at 8:00 and 20:00. In the case of normal rain gauge, the observation data are supplemented by dsj2 rain gauge in flood season.
Data quality description
The self recording rain gauge shall be calibrated before the beginning of flood season every year. 】In the observation process, when the abnormal value of the self recording rain gauge occurs, the ordinary rain gauge observation value is used for interpolation and verification; during the data entry process, four levels of manual verification are carried out, including tabulation, primary calibration, re calibration and audit, so as to ensure the data quality. 
Base information
collect time:2020/11/11-2010/12/31
collect place:Qiaogou watershed, Suide County, Yulin City, Shaanxi Province 
data size:332.9 KiB
data format:xls，doc，pdf
Coordinate system: 无 
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