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Datasets description
This table is the water level data of Tianshui rainfall test. The data is the data of ytyl0301 water level sensor, which is collected by TH302 acquisition instrument. The recording start and end time is 2020-07-16 to 2020-08-14. The acquisition interval is 3 minutes. The water depth resolution is 1cm. The data is stored in Excel. The data of four test pits are recorded, and each test pit has a sensor. 
Data source description
  Data acquisition is carried out by TH302 acquisition instrument.
Data processing method
  Using origin mapping, the data comes from rainfall, and the rainfall data in the whole process of rainfall test are obtained.
Data quality description
  Good data quality. 
Base information
collect time:2020/07/16-2020/08/15
collect place:Luoyugou watershed, Tianshui City, Gansu Province 
data size:4.5 MiB
data format:
Coordinate system: 无 
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