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Datasets description
 
Data source description
Artificial timing observation
Data processing method
1. Water level observation: Jiuyuangou runoff station uses the water gauge on the side wall of the building to measure the water level. In non flood season, the water level is observed once at 8:00 a.m. in case of rainfall, the daily water level changes slowly twice at 8:00 and 20:00; when the daily water level changes greatly or there is a slow peak and valley, it is observed four times at 2:00, 8:00, 14:00 and 20:00. When the water level changes violently in flood season, the observation shall be made in multiples of 6 minutes. 2. Flow measurement method: when the water level is higher than the delta channel, the flow measurement method is adopted in the rectangular spillway, and the buoy coefficient is the buoy test results of huangweizizhou runoff test station. 3. Sediment sampling and treatment: the midstream buoy method is used to sample the sediment at the flow measurement section. The frequency of sediment sampling depends on the frequency of flood water level change, and the sampling frequency is increased to control the change of sediment concentration at flood peak. The sample was treated by displacement method.
Data quality description
Manual observation is carried out by professional and technical personnel; four levels of manual verification are carried out in the process of data input, which are tabulation, initial calibration, re calibration and audit, so as to ensure the data quality. 
Base information
collect time:1991/01/01-2000/12/31
collect place:Jiuyuangou watershed, Suide County, Yulin City, Shaanxi Province 
altitude:2.0m- Nonem
data size:331.1 KiB
data format:xls，doc，pdf
Coordinate system: WGS84 
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