[SRTM]
SRTM V4

Original resolution: 3 arcsec (~90m)
Date of acquisition: February 2000
Date range: 2000-2000

# Data Citation

We kindly ask  any users to  cite this data  in any published  material
produced using this data, and if possible link web pages to the CIAT-CSI
SRTM website (http://srtm.csi.cgiar.org).

Citations should be made as follows: 

Jarvis A., H.I. Reuter, A.  Nelson, E. Guevara, 2008, Hole-filled seamless SRTM
data V4, International  Centre for Tropical  Agriculture (CIAT), available
from http://srtm.csi.cgiar.org,
  
[DEM3]
VIEWFINDER PANORAMAS DEMs

Original resolution: 3 arcsec (~90m)
Date of acquisition: Depending on original source

These data are downloaded from Jonathan de Ferranti's webpage:
http://viewfinderpanoramas.org/dem3.html

# Data Citation

There is no recommended citation for these data. Please refer to the website
above in case of doubt.

[RAMP]
RAMP V2

Original resolution: 200m
Date of acquisition: 1940-1999 (mostly 1980s and 1990s)
Date range: 1980-1990

Downloaded by F. Maussion from http://nsidc.org/data/nsidc-0082 on 28.03.2018

# Data Citation

As a condition of using these data, you must cite the use of this data set
using the following citation:

Liu, H., K. C. Jezek, B. Li, and Z. Zhao. 2015. Radarsat Antarctic Mapping
Project Digital Elevation Model, Version 2. Boulder, Colorado USA.
NASA National Snow and Ice Data Center Distributed Active Archive Center.
doi: https://doi.org/10.5067/8JKNEW6BFRVD. [28.03.2018].

[GIMP]
GIMP V1.1

Original resolution: 90 m
Date of acquisition: February 2003 - October 2009
Date range: 2003-2009

Downloaded by F. Maussion from http://nsidc.org/data/nsidc-0645/ on 28.03.2018

# Data Citation

As a condition of using these data, you must cite the use of this data set
using the following citation:

Howat, I., A. Negrete, and B. Smith. 2015. MEaSUREs Greenland Ice Mapping
Project (GIMP) Digital Elevation Model, Version 1.1. Boulder, Colorado USA.
NASA National Snow and Ice Data Center Distributed Active Archive Center.
doi: https://doi.org/10.5067/NV34YUIXLP9W. [28.03.2018].

# Literature Citation

As a condition of using these data, we request that you acknowledge the
author(s) of this data set by referencing the following peer-reviewed
publication:

Howat, I., A. Negrete, and B. Smith. 2014. The Greenland Ice Mapping Project
(GIMP) land classification and surface elevation data sets, The Cryosphere.
8. 1509-1518. https://doi.org/10.5194/tc-8-1509-2014

[ARCTICDEM]
ARCTICDEM V3

Original resolution: 100m
Date of acquisition: 2007-2018
Date range: 2007-2018

Downloaded by F. Maussion from http://data.pgc.umn.edu/elev/dem/setsm/ArcticDEM
on 24.05.2019 and split into 1 degree tiles.
See https://oggm.org/2019/10/08/dems/ for more information.

# Acknowledgements

These remarks should be included in the acknowledgements section of any
published work, presentation, poster, or document:

DEMs provided by the Polar Geospatial Center under NSF-OPP awards 1043681,
1559691, and 1542736.

# Data citation

As a condition of using these data, you must cite the use of this data set
using the following citation:

Porter, Claire; Morin, Paul; Howat, Ian; Noh, Myoung-Jon; Bates, Brian;
Peterman, Kenneth; Keesey, Scott; Schlenk, Matthew; Gardiner, Judith;
Tomko, Karen; Willis, Michael; Kelleher, Cole; Cloutier, Michael; Husby, Eric;
Foga, Steven; Nakamura, Hitomi; Platson, Melisa; Wethington, Michael, Jr.;
Williamson, Cathleen; Bauer, Gregory; Enos, Jeremy; Arnold, Galen;
Kramer, William; Becker, Peter; Doshi, Abhijit; D’Souza, Cristelle;
Cummens, Pat; Laurier, Fabien; Bojesen, Mikkel, 2018, “ArcticDEM”,
https://doi.org/10.7910/DVN/OHHUKH, Harvard Dataverse, V1, [Date Accessed]

[AW3D30]
AW3D30 V1804

Original resolution: 30m
Date of acquisition: 2006-2011
Date range: 2006-2011

# Terms of Use for ALOS Global Digital Surface Model (AW3D30)

- When you provide or publish any products and services to a third party using
this dataset, you are kindly requested to display that the original data is
provided by JAXA.
- When you publish the product(s) using this dataset, you are kindly requested
to show the copyright (©JAXA) and the source of data.
- JAXA does not guarantee the quality and reliability of this dataset and JAXA
assume no responsibility whatsoever for any direct or indirect damage and loss
caused by use of this dataset. Also, JAXA will not be responsible for any
damages of users due to changing, deleting or terminating the provision of this
dataset.

[MAPZEN]
MAPZEN TERRAIN TILES

Original resolution: variable
Date of acquisition: Depending on original source

A collection of DEMs from various sources hosted on Amazons Webs Service.
https://github.com/tilezen/joerd/tree/master/docs

# Attribution

Attribution is required for most original data sources. Please refer to the
Mazen attribution page for more information:
https://github.com/tilezen/joerd/blob/master/docs/attribution.md

[ASTER]
ASTGTMV3

Original Resolution: 1 arc second (~30m at the equator)
Date of acquisition: 2000 - 2013
Date range: 2000-2013

# Literature Citation

NASA/METI/AIST/Japan Spacesystems, and U.S./Japan ASTER Science Team (2019).
ASTER Global Digital Elevation Model V003 [Data set]. NASA EOSDIS Land
Processes DAAC. Accessed 20xx-x-x from https://doi.org/10.5067/ASTER/ASTGTM.003

[TANDEM]
TanDEM-X 90m

Original resolution: 90m
Date of acquisition: December 2010 - January 2015
Date range: 2011-2014

To access TanDEM-X data self-registration is necessary. Read and follow:
https://geoservice.dlr.de/web/dataguide/tdm90/#access
Afterwards use `oggm_netrc_credentials` to store your credentials locally.

# Data rights

In publications based on the TanDEM-X 90m DEM the User undertakes to clearly
mark all data in such a way that the authorship and copyright of DLR is
comprehensible to all: “© DLR ”. Derived information must include a reference
to the TanDEM-X 90m DEM as data source, regardless of the form in which it was
created.

# Data citation

Citation of one of the two listed papers is adequate if you use the TanDEM-X

Wessel, B., Huber, M., Wohlfart, C., Marschalk, U., Kosmann, D., Roth, A.
(2018): Accuracy Assessment of the Global TanDEM-X Digital Elevation Model with
GPS Data., ISPRS Journal of Photogrammetry and Remote Sensing. Vol. 139, pp.
171-182.

Rizzoli, P., Martone, M., Gonzalez, C., Wecklich, C., Borla Tridon, D.,
Bräutigam, B., Bachmann, M., Schulze, D., Fritz, T., Huber, M., Wessel, B.,
Krieger, G., Zink, M., and Moreira, A. (2017): Generation and performance
assessment of the global TanDEM-X digital elevation model. ISPRS Journal of
Photogrammetry and Remote Sensing, Vol 132, pp. 119-139.

[REMA]
REMA V1.1

Original resolution: 100m
Date of acquisition: 2009 - 2017 (mostly 2015-2016)
Date range: 2015-2016

Downloaded by F. Maussion from http://data.pgc.umn.edu/elev/dem/setsm/REMA
on 24.05.2019 and split into 1 degree tiles.
See https://oggm.org/2019/10/08/dems/ for more information.

# Acknowledgements

These remarks should be included in the acknowledgements section of any
published work, presentation, poster, or document:

DEMs provided by the Byrd Polar and Climate Research Center and the Polar
Geospatial Center under NSF-OPP awards 1543501, 1810976, 1542736, 1559691,
1043681, 1541332, 0753663, 1548562, 1238993 and NASA award NNX10AN61G. Computer
time provided through a Blue Waters Innovation Initiative. DEMs produced using
data from DigitalGlobe, Inc.

# Data citation

As a condition of using these data, you must cite the use of this data set
using the following citation:

Howat, I. M., Porter, C., Smith, B. E., Noh, M.-J., and Morin, P.:
The Reference Elevation Model of Antarctica, The Cryosphere, 13, 665-674,
https://doi.org/10.5194/tc-13-665-2019, 2019.

[ALASKA]
ALASKA V3

Original resolution: 30m
Date of acquisition: 2000-2011
Date range: 2000-2011

Provided by Christian Kienholz.

# Acknowledgements

These remarks should be included in the acknowledgements section of any
published work, presentation, poster, or document:

DEMs provided by Christian Kienholz.

# Data citation

As a condition of using these data, you must cite the use of this data set
using the following citation:

 Kienholz, C., Rich, J. L., Arendt, A. A., and Hock, R.: A new method for
 deriving glacier centerlines applied to glaciers in Alaska and northwest
 Canada, The Cryosphere, 8, 503–519, https://doi.org/10.5194/tc-8-503-2014,
 2014.

[COPDEM90]
Copernicus DEM GLO-90

Original resolution: 3 arc seconds (~90m)
Date of acquisition: 2010-2015
Date range: 2010-2015

# Credit

The GLO-90 dataset is available worldwide with a free license.

Full licences are available here:
https://spacedata.copernicus.eu/documents/20123/121286/CSCDA_ESA_Mission-specific+Annex_31_Oct_22.pdf/fb109818-56ad-bbee-053c-d972aed25ce6?t=1674741175657

ESA – EU users who use the Copernicus DEM in their research are requested
to use the following DOI when citing the data source in their publications:

    https://doi.org/10.5270/ESA-c5d3d65


[COPDEM30]
Copernicus DEM GLO-30

Original resolution: 1 arc seconds (~30m)
Date of acquisition: 2010-2015
Date range: 2010-2015

# Credit

The GLO-30 dataset is available worldwide with a free license
with the exception of two countries (Armenia and Azerbaijan).

Full licences are available here:
https://spacedata.copernicus.eu/documents/20123/121286/CSCDA_ESA_Mission-specific+Annex_31_Oct_22.pdf/fb109818-56ad-bbee-053c-d972aed25ce6?t=1674741175657

ESA – EU users who use the Copernicus DEM in their research are requested
to use the following DOI when citing the data source in their publications:

    https://doi.org/10.5270/ESA-c5d3d65

[NASADEM]
NASADEM Merged DEM Global

Original resolution: 1 arcsec (~30m)
Date of acquisition: February 2000
Date range: 2000-2000

# Data Citation

NASADEM Merged DEM Global 1 arc second - NASADEM_HGT
NASA JPL (2020). NASADEM Merged DEM Global 1 arc second V001 [Data set]. NASA
EOSDIS Land Processes DAAC. Accessed YYYY-MM-DD from
https://doi.org/10.5067/MEaSUREs/NASADEM/NASADEM_HGT.001
