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Datasets description
<p>&emsp;&emsp; This data set combines the characteristics of deep rock engineering with high geostress and high water head pressure to study the permeability evolution law of rocks under high confining pressure and high pore water pressure. Tight sandstone is selected to carry out seepage tests with variable pore water pressure under different confining pressure conditions. The permeability, deformation and other parameters of tight sandstone are measured by self-developed THMC multi field coupling test system. 
Data source description
<p>&emsp;&emsp; The data comes from the test measurement.
Data processing method
<p>&emsp;&emsp; The permeability and deformation of tight sandstone are measured by THMC multi field coupling test system.
Data quality description
<p>&emsp;&emsp; The data quality is good. 
Base information
collect time:2019/09/01-2019/09/30
collect place:Wuhan, Hubei 
data size:25.6 KiB
data format:
Coordinate system: 无 
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In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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