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Datasets description
 
Data source description
Field survey, image interpretation
Data processing method
Based on the fusion remote sensing image with spatial resolution of 2m, combined with the remote sensing image interpretation marks established by field investigation, the land use types such as dam land and terrace in the basin are extracted by manual visual interpretation using ArcGIS software platform.
Data quality description
Good 
Base information
collect time:2024/01/01-2024/12/31
collect place:Xindiangou watershed, Suide County, Yulin City, Shaanxi Province 
data size:801.7 KiB
data format:xls，pdf
Coordinate system: WGS84 
Keywords
Theme:Land use, underlying surface, water and soil conservation
	Subject:
	Time:2024
	Place:Xindiangou,  Suide,  Yulin,  Shaanxi Province 
Space scope
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	east：110.30

	
	south： 37.49
	


Service information
contacts: 
phone:0931-4967596
mailbox:ncdc@lzb.ac.cn
Contact information
contributors:Suide administration and Supervision Bureau of water and soil conservation of the Yellow River (Suide scientific experimental station of water and soil conservation) 
author:Suide administration and Supervision Bureau of water and soil conservation of the Yellow River (Suide scientific experimental station of water and soil conservation)  
manager:Suide administration and Supervision Bureau of water and soil conservation of the Yellow River (Suide scientific experimental station of water and soil conservation) 
Project information

Citations and annotations
In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
Data reference:
Suide administration and Supervision Bureau of water and soil conservation of the Yellow River (Suide scientific experimental station of water and soil conservation). Observation dataset of underlying surface in Xindiangou watershed, the first sub area of loess hilly and gully region in 2024. National Cryosphere Desert Data Center(http://www.ncdc.ac.cn), 2025. https://cstr.cn/CSTR:11738.11.NCDC.HWSDZHAN.DB6979.2025.




