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Datasets description
On July 25, 2012, lidar aerial remote sensing flight test was carried out in hulugou observation area in the middle and upper reaches of Heihe River by using Yun 12 aircraft and als70 produced by Leica company. The als70 laser has a wavelength of 1064nm and multiple echoes (1, 2, 3 and last) Hulugou area is divided into two flying areas with different altitudes. The absolute altitude is 4800 and 5500 meters, and the average point cloud density is 1 point / m2. Through the steps of parameter calibration, automatic classification of point cloud and manual editing, DSM and DEM data products are finally formed 
Data source description
  On July 25, 2012, lidar aerial remote sensing flight test was carried out in hulugou observation area in the middle and upper reaches of Heihe River by using Yun 12 aircraft and als70 produced by Leica company. The als70 laser has a wavelength of 1064nm and multiple echoes (1, 2, 3 and last)  Hulugou area is divided into two flying areas with different altitudes. The absolute altitude is 4800 and 5500 meters, and the average point cloud density is 1 point / m2
Data processing method
 DEM and DSM data products are finally formed through the steps of parameter calibration, automatic classification of point cloud and manual editing
Data quality description
 Good data quality 
Base information
collect time:2012/07/25-2012/07/26
collect place:Heihe River Basin, upstream cold region, hydrological test area, hulugou small watershed 
data size:200.2 MiB
data format:las
Coordinate system: WGS84 
Projection / 
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	Place:Heihe River Basin,  Hulugou small watershed,  Hydrological test area in upper cold region 
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For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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