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Datasets description
This data set is the underlying surface observation data set of peijiamaogou watershed in the first sub area of Loess Hilly and gully region from 2021 to 2022. The data set is based on the remote sensing images of "gaogao-1" satellite in 2021 and 2022. The remote sensing images are interpreted by ArcGIS software, supplemented by field investigation, and the attributes and boundaries of the interpreted spots are verified and corrected one by one. This data set includes the land use status table of peijiamaogou watershed, the thematic map of land use of peijiamaogou watershed and the underlying surface investigation report 
Data source description
Field research, image interpretation
Data processing method
Based on the fusion remote sensing image with spatial resolution of 2m, combined with the remote sensing image interpretation marks established by field investigation, the land use types such as dam land and terrace in the basin are extracted by manual visual interpretation using ArcGIS software platform.
Data quality description
Good 
Base information
collect time:2021/01/01-2022/12/31
collect place:Peijiamaogou watershed, Suide County, Yulin City, Shaanxi Province 
data size:14.7 MiB
data format:
Coordinate system: WGS84 
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Citations and annotations
In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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