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Datasets description
This data set is the data of sedimentation survey of Huaguoshan reservoir in 1964-1978, 1980-1981 and 2011-2017 in Nanxiaohegou basin. The sedimentation section method is used to measure the deposition of about 200 measuring points in 7 deposition sections of main channel and 6 deposition sections of branch channel. Generally, the erosion modulus is calculated by observing the elevation of the silting surface at each section before, after or after the flood season. 
Data source description
Artificial timing observation
Data processing method
The sedimentation section method is used to measure the deposition of about 200 measuring points in 7 deposition sections of main channel and 6 deposition sections of branch channel. Generally, the observation is conducted before, after or after the flood season. Firstly, the elevation of the deposition surface at each section is observed, and then the deposition amount is calculated in sections. Finally, the erosion modulus of the basin above the Huaguoshan reservoir is calculated.
Data quality description
In the process of compilation and input of observation data, there are four levels of manual verification, including tabulation, primary calibration, recheck and audit, so as to ensure the data quality. 
Base information
collect time:1964/01/01-2017/12/31
collect place:Nanxiaohegou watershed, houguanzhai Township, Xifeng District, Qingyang City, Gansu Province 
altitude:1050.0m- 1423.0m
data size:4.9 MiB
data format:
Coordinate system: 无 
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