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Datasets description
The dataset is the groundwater survey data of the Hailiutu River Basin in Ordos City, Inner Mongolia Autonomous Region. It includes the latitude, longitude, elevation, and groundwater depth of the main control points and logging wells. The data measurement is recorded using handheld GPS. It can analyze the groundwater flow field, burial depth, and underground characteristics of the groundwater aquifer in the basin. 
Data source description
    Actual measurement, generated independently.
Data processing method
    Handheld GPS is used to record location and elevation, and water level is recorded by a measuring rope.
Data quality description
    The data quality is good. 
Base information
collect time:2019/04/01-2019/06/30
collect place:Hailiutu River Basin, Ordos City, Inner Mongolia Autonomous Region 
data size:175.0 KiB
data format:Excel
Coordinate system: 无 
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