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Datasets description
This dataset contains (1) Gansu Zhangye CASI + Sasi aerial remote sensing data processing （2）Process of the airborne data_ CASI+SASI On June 29, 2012 and July 7, 2012, in the 30 * 30km core observation area and the midstream sample zone in the middle reaches of Heihe River, the flight test of obtaining visible / near-infrared short wave infrared hyperspectral aerial remote sensing data was carried out by using Yun 12 aircraft and CASI / Sasi sensors. The relative flight altitude is 2000 meters (altitude is 3500 meters). The wavelength ranges of CASI and Sasi sensors are 380-1050 nm and 950-2450 nm respectively, and the spatial resolution is 1 meter and 2.4 meters respectively. The surface reflectance product is obtained by using the synchronously measured ground data and atmospheric data through geometric and 6S atmospheric correction 
Data source description
  On June 29, 2012 and July 7, 2012, in the 30 * 30km core observation area and the midstream sample zone in the middle reaches of Heihe River, the flight test of obtaining visible / near-infrared short wave infrared hyperspectral aerial remote sensing data was carried out by using Yun 12 aircraft and CASI / Sasi sensors
Data processing method
  The relative flight altitude is 2000 meters (altitude is 3500 meters). The wavelength ranges of CASI and Sasi sensors are 380-1050 nm and 950-2450 nm respectively, and the spatial resolution is 1 meter and 2.4 meters respectively. The surface reflectance product is obtained by using the synchronously measured ground data and atmospheric data through geometric and 6S atmospheric correction
Data quality description
 Good data quality 
Base information
collect time:2012/06/29-2012/06/30
collect place:
data size:302.9 GiB
data format:
Coordinate system: WGS84 
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	Subject:remote sensing geology 
	Time:2012
	Place:Artificial oasis experimental area in the middle reaches,  Heihe River Basin 
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Citations and annotations
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For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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