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Datasets description
This data product (L7 SLC off) refers to the abnormal data product after Landsat 7 SLC failure on May 31, 2003 The Landsat ETM + remote sensing data set passed the joint experiment of comprehensive remote sensing observation of ecological hydrological process in Heihe River Basin http://glovis.usgs.gov/ Download for 
Data source description
 Landsat-7 was launched on April 15, 1999. Its main sensor is enhanced thematic imager (ETM +). In addition to maintaining the basic consistency with Landsat-5 in terms of spatial resolution and spectral characteristics, Landsat-7 has added many new features, which has been widely valued and welcomed by users all over the world. Since its launch, it has provided users with a large number of high-quality image data. Landsat-7 scans the same area every 16 days, that is, it covers the world once every 16 days
Data processing method
 Landsat ETM + image data includes 8 bands. The spatial resolution of band1-band5 and band7 is 30m, that of Band6 is 60m and that of band8 is 15m.  In 2012, 5 Landsat ETM + images were obtained. The coverage is the ecological and hydrological test area of artificial oasis in the middle reaches, and the acquisition time (Beijing time) is: 2012-04-05, 2012-04-21, 2012-05-07, 2012-06-242012-07-10.  The transit time of the above data is about 11:50 (Beijing time)
Data quality description
 Good data quality 
Base information
collect time:2012/04/05-2012/07/10
collect place:Heihe River Basin 
data size:1.3 GiB
data format:jpg
Coordinate system: WGS84 
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Citations and annotations
In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
For the achievements published in English, please refer to the following specifications：
The dataset is provided by National Cryosphere Desert Data Center(https://www.ncdc.ac.cn).
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